| ManualsContentsPreviousNext |

# Configuring the Network Interface Board

Use the following command to display network interface board settings:

- telnet : Use the "show" command.

Protocol Up/Down

The following protocols are displayed ("Up" indicates enabled; "Down" indicates disabled):

IPv4, IPv6, IPsec, NetWare, SMB

Device Up/Down

The following device is displayed ("Up" indicates enabled; "Down", indicates disabled):

USB

Ethernet interface

Displays the Ethernet speed.

Syslog priority

"LOG_INFO" is displayed.

NVRAM version

Displays the NVRAM version.

Device name

Displays the device name.

Comment

Displays the comment(s).

Location

Displays the location of the device.

Contact

Displays the contact details.

Soft switch

Displays the soft switch.

TCP/IP

The following items are displayed: ("Up" indicates enabled; "Down", indicates disabled):

- Mode(IPv4)

- Mode(IPv6)

  ftp, lpr, rsh, diprint, web, http, ftpc, snmp, ipp, autonet, Bonjour, ssl, nrs, rfu, nbt, ssdp, ssh, sftp, WSD (Device), WSD (Printer), WSD (Scanner), rhpp

- IPv4

  DHCP, Address, Netmask, Broadcast, Gateway

- IPv6

  Stateless, Manual, Gateway, DHCPv6-lite, DUID, DHCPv6 option lifetime

- IPsec

  Manual Mode, Excluded Protocol (https, dns, dhcp, wins)

- EncapType

- Host name

- DNS Domain

- Access Control

  IPv4: Access Entry [1]-[5]

  IPv6: Access Entry [1]-[5]

- SNTP Server

- Time Zone

- SNTP Server polling time

- SYSLOG server

- Home page URL1

- Home page link name1

- Home page URL2

- Home page link name2

- Help page URL

- RHPP Port

- RHPP timeout

NetWare

The following items are displayed:

- EncapType

- RPRINTER number

- Print server name

- File server name

- Context name

- Switch

  Mode, NDS/Bindery, Packet negotiation, Login Mode

- Print job timeout

- Protocol

- SAP interval time

- NDS Tree Name

- Transfer Protocol

SMB

The following items are displayed:

- Switch

  Mode, Direct print, Notification

- Workgroup name

- Computer name

- Comment

- Share name[1]

- Protocol

Wireless LAN

The following items are displayed:

Host name, Communication Mode, SSID, Channel, Security, WEP Authentication, WEP Encryption key number, WEP Encryption keys [1]-[4], WPA Encryption, WPA Authentication, Pre-Shared Key, User name, Domain name, EAP Type, Password, Phase 2 user name, Phase 2 Method TTLS, Phase 2 Method PEAP, Server cert., Intermediate CA, Server ID, Sub domain, Mic check

Ethernet

The following item is displayed:

802.1X Authentication

DNS

The following items are displayed:

- IPv4

  Server[1]-[3], Selected IPv4 DNS Server

- IPv6

  Server[1]-[3], Selected IPv6 DNS Server, Resolver Protocol

Domain name

The following items are displayed:

ether, wlan

DDNS

The following items are displayed:

ether, wlan

WINS

The following items are displayed:

- ether

  Primary WINS, Secondary WINS

- wlan

  Primary WINS, Secondary WINS

SSDP

The following items are displayed:

UUID, Profile, TTL

UPnP

The following item is displayed:

URL

Bonjour

The following items are displayed:

Computer Name(cname), Local Hostname(ether), Local Hostname(wlan), Location, Priority(diprint), Priority(lpr), Priority(ipp), IP TTL, LinkLocal Route for Multi I/F, IPP Port

SNMP

The following items are displayed:

SNMPv1v2, SNMPv3, protocol, v1Trap, v2Trap, v3Trap, SNMPv1v2 Remote Setting, SNMPv3 Privacy

ssh

The following items are displayed:

Compression, Port, TimeOut, LoginTimeOut

AuthFree

The following items are displayed:

- IPv4

  AuthFree Entry [1]-[5]

- IPv6

  AuthFree Entry [1]-[5]

- USB

LPR

The following items are displayed:

lprm check host, lpr prnerrchk

Certificate

The following item is displayed:

Verification

WS-MFP

The following items are displayed:

Network Device Name, Comments, Location, Presentation URL, WSD (Device) TCP Port, WSD (Printer) TCP Port, WSD (Printer) Job Timeout, WSD (Scanner) TCP Port, MetadataVersion, UUID

IEEE 802.1X

The following items are displayed:

User name, Domain name, EAP Type, Password, Phase 2 user name, Phase 2 Method TTLS, Phase 2 Method PEAP, Server cert., Intermediate CA, Server ID, Sub domain

Shell mode

"User mode" is displayed.