| ManualsContentsPreviousNext |

# Handling the machine's interior

This section explains safety precautions about handling the machine's interior.

| Do not remove any covers or screws other than those explicitly mentioned in this manual. Inside this machine are high voltage components that are an electric shock hazard and laser components that could cause blindness. Contact your sales or service representative if any of the machine's internal components require maintenance, adjustment, or repair. Do not attempt to disassemble or modify this machine. Doing so risks burns and electric shock. Note again that exposure to the laser components inside this machine risks blindness.

| Be sure to turn off the power switch and wait for about 15 minutes before cleaning the registration roller. Not waiting for the machine to cool down can result in a burn.

| Some of this machine's internal components get very hot. For this reason, take care when removing misfed paper. Not doing so could result in burns.

| The inside of the machine could be very hot. Do not touch the parts with a label indicating the “hot surface”. Otherwise, an injury might occur.

| When loading paper, take care not to trap or injure your fingers.

| During operation, rollers for transporting the paper and originals revolve. A safety device has been installed so that the machine can be operated safely. But take care not to touch the machine during operation. Otherwise, an injury might occur.

| If the machine's interior is not cleaned regularly, dust will accumulate. Fire and breakdown can result from heavy accumulation of dust inside this machine. Contact your sales or service representative for details about and charges for cleaning the machine's interior.

| The fusing section of this machine might be very hot. Caution should be taken when removing misfed paper.

| Lifting the paper feed unit carelessly or dropping it may cause injury.

| Do not pull out the paper tray forcefully. If you do, the tray might fall and cause an injury.