| ManualsContentsPreviousNext |

# Placing Originals

To correctly display the top/bottom orientation of the scanned original on a client computer, the placement of the original and the settings made on the control panel must match.

Place originals correctly by referring to the following tables:

Exposure Glass

Place the original face down on the exposure glass in either the up-down (portrait) or left-right (landscape) orientation.

Original orientation and control panel key selection
Original orientation | Control panel key
--- | ---
top edge touches top left corner of exposure glass |
top edge touches rear of exposure glass |

ADF

Hold the original so that its text is in the natural readable orientation, and then place it face up in the ADF.

Original orientation and control panel key selection
Original orientation | Control panel key
--- | ---
top edge placed first |
top edge touches rear of ADF |

- When you specify full color, gray scale, or [Auto Colour Select] for Original Type, and single page TIFF/JPEG or multi-page TIFF is selected as the file type, refer to the tables below for how to place originals. Originals placed in orientations that are not recommended in the table might appear incorrectly top/bottom oriented on client computer displays.

  Exposure glass
  Original orientation | Control panel key
  --- | ---
  top edge touches top left corner of exposure glass |

  ADF
  Original orientation | Control panel key
  --- | ---
  top edge placed first |