ManualsContentsPreviousNext
Settings

# Booklet/Magazine

Copies two or more originals in page order.

- You cannot use the bypass tray with this function.

There are four types of Booklet/Magazine.

1 Sided Booklet

Make copies in page order for a folded booklet as shown.

1. Open to left

2. Open to right

2 Sided Booklet

Make 2-sided originals to copies in page order for a folded booklet as shown.

1. Open to left

2. Open to right

1 Sided Magazine

Copies two or more originals to make copies in page order when they are folded and stacked.

1. Open to left

2. Open to right

2 Sided Magazine

Copies two or more originals of 2-sided to make copies in page order when they are folded and stacked.

1. Open to left

2. Open to right

How to fold and unfold copies to make a booklet

Fold a copy along the centerline, and open.

1. Open to left

2. Open to right

How to fold and unfold copies to make a magazine

Fold and stack copies to make a magazine, and open.

1. Open to left

2. Open to right

Press [Original Settng].

Press [Original Size].

Specify the original size, and then press [OK].

Select original orientation.

Press [OK].

Press [Dup./Combine/Series].

Press [Book].

Select a book type separately for the original ([1 Sided] or [2 Sided]) and copy ([Booklet] or [Magazine]).

If you specified [2 Sided] for the original, you can specify the orientation of originals or copies. For details, see “Originals and Copy Orientation”.

Press [OK].

Select the paper tray.

- When placing originals on the exposure glass, or in the ADF using Batch mode, press the [] key after all the originals have been scanned.

- The default setting for the orientation of Booklet and Magazine is [Open to Left]. You can change the default under Orientation: Booklet, Magazine in User Tools. For details, see “Edit”.

- In the Booklet or Magazine mode, the machine sets the reproduction ratio automatically to meet the paper size and copies the originals together onto the paper.

- The machine selects reproduction ratios of between 25 and 400%. However, if the originals are placed in the ADF, the maximum reproduction ratio is 200%. To copy originals at a reproduction ratio above 200%, you must place them on the exposure glass.

- If the calculated ratio is under the minimum ratio, it is automatically adjusted to within available range. However, with some ratios, parts of the image might not be copied.

- Depending on the orientation of the original and copy paper, the machine will automatically rotate the image by 90 degrees to make copies properly.

- You cannot copy with originals different in size and orientation.

- If the number of originals scanned is less than a multiple of 4, the last page is copied blank.

- In Magazine mode, the copying may take some time after scanning originals.

- Originals and Copy Orientation

- Edit