ManualsContentsPreviousNext
Settings

# Sending originals using the exposure glass (Immediate Transmission)

This section explains how to send originals by Immediate Transmission using the exposure glass.

Press [Immed. TX].

Place the first page face down on the exposure glass.

Specify a destination.

Make the scan settings you require.

Press the [Start] key.

The machine dials the destination.

Place the next original on the exposure glass within 10 seconds when you send multiple originals, and then repeat steps 4 and 5.

Repeat this step for each page.

Press the [] key.