ManualsContentsPreviousNext
Settings

# Ethernet

This section lists the settings required for delivering data to the network with an Ethernet connection.

For details about how to specify the settings, see "Interface Settings" and "File Transfer".

Menu | User Tool | Setting Requirements
--- | --- | ---
Interface Settings/Network | Machine IPv4 Address | Necessary
Interface Settings/Network | IPv4 Gateway Address | As required
Interface Settings/Network | Machine IPv6 Address | As required
Interface Settings/Network | IPv6 Gateway Address | As required
Interface Settings/Network | IPv6 Stateless Address Autoconfiguration | As required
Interface Settings/Network | DNS Configuration | As required
Interface Settings/Network | DDNS Configuration | As required
Interface Settings/Network | IPsec | As required
Interface Settings/Network | Domain Name | As required
Interface Settings/Network | WINS Configuration | As required
Interface Settings/Network | Effective Protocol | Necessary
Interface Settings/Network | Ethernet Speed | As required
Interface Settings/Network | LAN Type | Necessary
Interface Settings/Network | Permit SNMPv3 Communication | As required
Interface Settings/Network | Permit SSL / TLS Communication | As required
Interface Settings/Network | Host Name | As required
Interface Settings/Network | IEEE 802.1X Authentication for Ethernet | As required
File Transfer | Delivery Option | Necessary
File Transfer | Fax RX File Transmission | As required
File Transfer | Scanner Resend Interval Time | As required
File Transfer | Number of Scanner Resends | As required

- For the Effective Protocol setting, check that the protocol you want to use is set to [Active].

- [LAN Type] is displayed when the wireless LAN board is installed. If both Ethernet and wireless LAN are connected, the selected interface takes precedence.

- If Delivery Option is set to [On], check that IPv4 Address is specified.

- Interface Settings

- File Transfer