ManualsContentsPreviousNext
Settings

# Memory Lock

Store incoming documents from programmed senders (Special Senders) in memory without printing them. People without the Memory Lock ID cannot print the documents, and therefore this function is useful for receiving confidential documents. If you do not program any senders, the machine receives fax document from all senders using Memory Lock reception.

- You must register Memory Lock ID in advance. For details about how to register Memory Lock ID, see “Initial Settings”.

- If you program the same sender in Memory Lock and Forwarding, Forwarding is disabled.

- Initial Settings