ManualsContentsPreviousNext
Settings

# Windows 7, Windows Server 2008 R2 - WSD port

Quit all applications currently running.

On the [Start] menu, click [Computer].

Click [Network].

Right-click the machine's icon, and then click [Install].

Driver installation starts automatically.

If the "Device driver software was not successfully installed" message appears, close the message, and then proceed to step 5.

On the [Start] menu, click [Devices and Printers].

Click [Add a printer].

Click [Add a local printer].

Check the [Use an existing port:] check box, and select WSD port.

Click [Next].

Click [Have Disk...].

Insert the CD-ROM into the CD-ROM drive.

If the [AutoPlay] dialog box appears, click the [Close] button.

Click [Browse...], and then specify a location for the printer driver.

If the CD-ROM drive is D, the source files of the printer driver are stored in the following locations:

- PCL 5e

  D:\x86 or X64\DRIVERS\PCL5e\XP_VISTA or X64\(Language)\DISK1

- PCL 6

  D:\x86 or X64\DRIVERS\PCL6\XP_VISTA or X64\MUI\DISK1

- PostScript 3

  D:\x86 or X64\DRIVERS\PS\XP_VISTA or X64\MUI\DISK1

The PCL 6 printer driver is installed in the language specified by your operating system.

Click [OK] to close the [Install From Disk] window.

Select the manufacturer and model name of the machine you want to use, and then click [Next].

Follow the instructions on the screens.

According to your needs, you may change the machine name, configure the machine as a default printer and/or a shared printer, and print a test page.

Click [Finish].

If installation is successful, the icon of the printer connected to the WSD port is added to the [Devices and Printers] window.

- The port name that follows "WSD" uses random character strings. It cannot be changed freely.

- To stop installation of the selected driver, click [Cancel] before the installation is complete. When re-installing the WSD Port, right-click the machine's icon in the [Network] window, and then click [Uninstall].