| ManualsContentsPreviousNext |

# Setting an Internet Fax/E-mail Destination as a BCC

E-mail is sent to all specified Internet Fax or e-mail destinations as bcc.

1. Place the original, and then select the scan settings you require.

2. Specify the sender.

   For details, see “Sender Settings”.

3. Press [TX Mode].

4. Press [BCC Transmission] to highlight it.

5. Press [OK].

   The standby display appears.

   To check the settings, press [TX Mode].

6. Specify a destination, and then press the [Start] key.

- You can program one of the Quick Operation keys with operations for this function. Using the Quick Operation Key allows you to omit steps 3 and 5. For details about Quick Operation Key, see “General Settings”.

- Sender Settings

- General Settings