ManualsContentsPreviousNext
Settings

# SEP Code Reception

Enable this function to perform SEP Code Reception.

- This function is not available with Internet Fax and e-mail.

- To perform SEP Code Reception, a SEP Code must be set in [Adv.Features], the Address Book, or Keystroke Programs in advance. Otherwise, even if “SEP Code Reception” is set to on, reception is not performed.

- When you select a destination that has a registered SEP Code from the Address Book, if “SEP Code Reception” is set to off, the SEP Code is not appended and transmission is in standard fax mode.

Press [TX Mode].

Select [Option Setting].

Press [SEP Code Reception] to highlight it.

To cancel SEP Code Reception, press [SEP Code Reception] again.

Press [OK] twice.

Specify the destination, and then press the [Start] key.

- For details about specifying SEP Codes, see the following:

  - To specify SEP Codes in “Adv.Features”, see “Setting SEP Codes for Reception”.

  - To register SEP Codes in the Address Book, see “Registering Addresses and Users for Facsimile/Scanner Functions”, Network and System Settings Reference.

  - To register SEP Codes in Keystroke Programs, see “Registering and Changing Keystroke Programs”.

- You can program one of the Quick Operation keys with operations for this function. Using the Quick Operation Key allows you to omit steps 1, 2, and 4. For details about Quick Operation Key, see “General Settings”.

- Setting SEP Codes for Reception

- General Settings

- Registering and Changing Keystroke Programs