ManualsContentsPreviousNext
Settings

# Installing the Board (Optional)

| Do not remove any covers or screws other than those explicitly mentioned in this manual. Inside this machine are high voltage components that are an electric shock hazard and laser components that could cause blindness. Contact your sales or service representative if any of the machine's internal components require maintenance, adjustment, or repair. Do not attempt to disassemble or modify this machine. Doing so risks burns and electric shock. Note again that exposure to the laser components inside this machine risks blindness.

| Keep the polythene materials (bags, gloves, etc.) supplied with this machine away from babies and small children at all times. Suffocation can result if polythene materials are brought into contact with the mouth or nose.

| When disconnecting the power cord from the wall outlet, always pull the plug, not the cord. Pulling the cord can damage the power cord. Use of damaged power cords could result in fire or electric shock.

| Before installing or removing options, always disconnect the power cord plugs from the wall outlet and allow time for the main unit to fully cool. Failing to take these precautions could result in burns.

| Wait at least one hour after power off before replacing parts. Not allowing the machine to cool may result in burns.

- Before beginning work, ground yourself by touching something metal to discharge any static electricity. Static electricity can damage the interface board.

- Do not subject the board to physical shocks.

Related topics

Installing the Gigabit Ethernet Board (mainly Europe and Asia)
Installing the Gigabit Ethernet Board (mainly North America)
Installing the Wireless LAN Interface Board
Installing the File Format Converter