ManualsContentsPreviousNext
Settings

# When the machine is connected to the computer using the interface cable

This section describes how to check the print port when the Data In indicator does not light up or blink.

Check if the print port setting is correct.

For Windows XP Professional or Windows Server 2003/2003 R2

1. Click the [start] button, and then click [Printers and Faxes].

2. Click the icon of the machine. On the [File] menu, click [Properties].

3. Click the [Ports] tab.

4. In the [Print to the following port(s)] list, confirm the correct port is selected.

For Windows XP Home Edition

1. Click the [start] button, and then click [Control Panel].

2. Click [Printers and Other Hardware].

3. Click [Printers and Faxes].

4. Click the icon of the machine. On the [File] menu, click [Properties].

5. Click the [Ports] tab.

6. In the [Print to the following port(s)] list, confirm the correct port is selected.

For Windows Vista

1. Click the Start button, and then click [Control Panel].

2. Click [Hardware and Sound].

3. Click [Printers].

4. Click the icon of the machine. On the [Organize] menu, click [Properties].

5. Click the [Ports] tab.

6. In the [Print to the following port(s)] list, confirm the correct port is selected.

For Windows 7

1. Click the Start button, and then click [Control Panel].

2. Click [Hardware and Sound].

3. Click [Devices and Printers].

4. Right click the icon of the machine. On the context menu, click [Printer properties].

5. Click the [Ports] tab.

6. In the [Print to the following port(s)] list, confirm the correct port is selected.

For Windows Server 2008

1. Click the [Start] button, and then click [Control Panel].

2. Click [Hardware and Sound].

3. Click [Printers].

4. Click the icon of the machine. On the [Organize] menu, click [Properties].

5. Click the [Ports] tab.

6. In the [Print to the following port(s)] list, confirm the correct port is selected.

For Windows Server 2008 R2

1. Click the [Start] button, and then click [Control Panel].

2. Click [Hardware].

3. Click [Devices and Printers].

4. Right click the icon of the machine. On the context menu, click [Printer properties].

5. Click the [Ports] tab.

6. In the [Print to the following port(s)] list, confirm the correct port is selected.