ManualsContentsPreviousNext
Settings

# Recommended Paper Sizes and Types

This section describes recommended paper sizes and types.

- Do not use paper designed for inkjet printers, as these may stick to the fusing unit and cause a misfeed.

- If you use damp or curled paper, a staple clogging or paper jam may occur.

Tray 1

Paper type and weight | Paper size | Paper capacity *1
--- | --- | ---
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that can be detected automatically: A4, A5, B5 JIS, 81/2 × 14, 81/2 × 11 A4, B5 JIS, 81/2 × 14, 81/2 × 11, 51/2 × 81/2 | 550 sheets
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that you need to specify*3: A5, A6, B6 JIS, 81/2 × 13, 81/4 × 13, 8 × 13, 71/4 × 101/2, 51/2 × 81/2, 16K A5, A6, B6 JIS, 81/2 × 13, 81/4 × 13, 8 × 13, 71/4 × 101/2, 51/2 × 81/2, 16K | 550 sheets
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that you need to enter*2: Vertical: 140.0 356.0 mm Horizontal: 98.0 216.0 mm Vertical: 5.52 14.01 inches Horizontal: 3.86 8.50 inches | 550 sheets
Envelopes *7 | Sizes of envelopes that you need to specify*3: 41/8 × 91/2, 37/8 × 71/2, C5 Env, C6 Env, DL Env | 10 sheets

Trays 2 4

Paper type and weight | Paper size | Paper capacity *1
--- | --- | ---
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that can be detected automatically: A4, A5, B5 JIS, 81/2 × 14, 81/2 × 11 A4, B5 JIS, 81/2 × 14, 81/2 × 11, 51/2 × 81/2 | 550 sheets
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that you need to specify*3: B6 JIS, 81/2 × 13, 81/4 × 13, 8 × 13, 71/4 × 101/2, 51/2 × 81/2, 16K A5, B6 JIS, 81/2 × 13, 81/4 × 13, 8 × 13, 71/4 × 101/2, 16K | 550 sheets
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that you need to enter*2: Vertical: 160.0 356.0 mm Horizontal: 98.0 216.0 mm Vertical: 6.30 14.01 inches Horizontal: 3.86 8.50 inches | 550 sheets
Envelopes *7 | Sizes of envelopes that you need to specify*3: 41/8 × 91/2, 37/8 × 71/2, C5 Env, C6 Env, DL Env | 10 sheets

Bypass tray

Paper type and weight | Paper size | Paper capacity *9
--- | --- | ---
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that you need to specify*4: A4, A5, A6, B5 JIS, B6 JIS, 81/2 × 14, 81/2 × 13, 81/2 × 11, 81/4 × 13, 8 × 13, 71/4 × 101/2, 51/2 × 81/2, 16K | 100 sheets
52 220 g/m2 14 lb. Bond 80 lb. Cover Thin Paper Thick Paper 3 | Paper sizes that you need to enter*5: Vertical: 140.0 900.0 mm Horizontal: 64.0 216.0 mm Vertical: 5.52 35.43 inches Horizontal: 2.52 8.50 inches | 100 sheets
OHP transparencies *6 | A4 | 100 sheets*8
Label paper (adhesive labels) | A4 | 1 sheet
Envelopes *7 | Paper sizes that you need to specify*4: 41/8 × 91/2, 37/8 × 71/2, C5 Env, C6 Env, DL Env | 10 sheets

*1 When loading paper, make sure the stack height does not exceed the limit mark of the paper tray.

*2 Enter the paper size under Tray Paper Size: Tray 1 4 in System Settings. See “System Settings”, Network and System Settings Reference.

*3 Select the paper size under Tray Paper Size: Tray 1 4 in System Settings. See “System Settings”, Network and System Settings Reference.

*4 Select the paper size. For details, see “Copying onto Regular Size Paper”, Copy and Document Server Reference, or “Setting the Paper Size Using the Control Panel”, Printer Reference.

*5 Enter the paper size using the number keys. For details, see “Copying onto Custom Size Paper”, Copy and Document Server Reference, or “Setting Custom Size Paper Using the Control Panel”, Printer Reference.

*6 Select [OHP (Transparency)] for paper type. For details, see “Copying onto OHP Transparencies or Thin Paper”, Copy and Document Server Reference, or “Setting Thick Paper, Thin Paper or OHP Transparencies Using the Control Panel”, Printer Reference.

*7 For details about loading envelopes, see “Envelopes”.

*8 It is recommended to place one sheet at a time when a misfeed occur.

*9 Load only as much paper as can be held between the paper guides on the bypass tray.

Paper Thickness

Paper Thickness *1 | Paper weight
--- | ---
Thin Paper | 52 59 g/m2 (14 16 lb. Bond)
Plain Paper 1 | 60 69 g/m2 (16 18 lb. Bond)
Plain Paper 2 | 70 90 g/m2 (19 24 lb. Bond)
Middle Thick | 91 105 g/m2 (24 28 lb. Bond)
Thick Paper 1 | 106 130 g/m2 (28 35 lb. Bond)
Thick Paper 2 | 131 163 g/m2 (35 lb. Bond 90 lb. Index)
Thick Paper 3 | 164 220 g/m2 (90 lb. Index 80 lb. Cover)

*1 Print quality will decrease if the paper you are using is close to the minimum or maximum weight. Change the paper weight setting to thinner or thicker.

- When loading paper in trays 1 4, place the print side down. When loading paper in the bypass tray, place the print side up.

- When loading thick paper, see “Thick Paper”.

- When using translucent paper or label paper, make sure to select the appropriate paper type under Paper Type: Bypass Tray. See “System Settings”, Network and System Settings Reference.

- Certain types of paper produce noise when delivered. This noise does not indicate a problem and print quality is unaffected. (OHP transparencies can produce noise when delivered.)

- When you load OHP transparencies, check the front and back of the sheets, and place them correctly, or a misfeed might occur. For details, see Copy and Document Server Reference, and Printer Reference.

- When you use OHP transparencies, fan them for each use.

- We recommend that you use a 4000 ANSI lumen or brighter overhead projector to project OHP transparencies.

- When copying or printing onto OHP transparencies or thick paper, the copy/print speed is slower than usual.

- Flatten out curled sheets before loading them.

- If multiple sheet feeding occurs, load sheets one by one.

- When copying or printing onto letterhead paper, the paper placing orientation is different depending on which function you are using. See “Loading Orientation-Fixed Paper or Two-Sided Paper”.

- If you load paper of the same size in two or more trays, the machine automatically shifts to the other tray when the first tray in use runs out of paper. This function is called Auto Tray Switching. (However, if the paper type of one tray is recycled or special paper, the settings of the other trays must be the same for the Auto Tray Switching function to work.) This saves interrupting a copy run to replenish paper when making a large number of copies. You can set the paper type of trays 1 4 under Paper Type: Tray 1 4. See “System Settings”, Network and System Settings Reference. For the setting procedure of the Auto Tray Switching function, see “Copier and Document Server Features”, Copy and Document Server Reference.

- Loading Orientation-Fixed Paper or Two-Sided Paper

- Envelopes

- Thick Paper