| ManualsContentsPreviousNext |

# Specifications for Wireless LAN Board (Optional)

Transmission spec.:

- (mainly Europe and Asia)

  - Based on IEEE 802.11a/b/g (wireless LAN)

  - Based on IEEE 802.11b/g (wireless LAN)

- (mainly North America)

  - Based on IEEE 802.11a/b/g (wireless LAN)

Protocol:

TCP/IP, IPX/SPX

Transmission Rate:

Auto select from the following speed:

1 Mbps, 2 Mbps, 5.5 Mbps, 6 Mbps, 9 Mbps, 11 Mbps, 12Mbps, 18Mbps, 24 Mbps, 36 Mbps, 48 Mbps, 54 Mbps

Frequency range (Center Frequency):

- (mainly Europe and Asia)

  - IEEE 802.11a/b/g wireless LAN:

    - 2412 2472 MHz (1 13 channels)

    - 5180 5320 MHz (36, 40, 44, 48, 52, 56, 60, and 64 channels)

  - IEEE 802.11b/g wireless LAN:

    - 2412 - 2462 MHz (1 - 11 channels)

- (mainly North America)

  - IEEE 802.11a/b/g wireless LAN:

    - 2412 2462 MHz (1 11 channels)

    - 5180 5320 MHz (36, 40, 44, 48, 52, 56, 60, and 64 channels)

Transmission mode:

- Ad hoc mode

- Infrastructure mode

- Web Image Monitor is supported.

- The channel in use might differ depending on the country.