| ManualsContentsPreviousNext |

# Sending Fax Documents from Computers

You can send a document created with a Windows application from a computer connected to the machine to another fax machine.

Connect computers to the machine via LAN, wireless LAN, or USB 2.0.

- To send a fax, simply select [Print...] from the Windows application, then select LAN-Fax as the printer, and then specify a destination. LAN-Fax enables paperless faxing from your computer to the other destinations.

- In addition to sending faxes, the LAN-Fax Driver allows this machine to be used for printing out documents prepared on a computer for proof checking.

- To use the LAN-Fax Driver, connect this machine to computers and make the necessary network settings, and then install the LAN-Fax Driver and the related utilities on your computer.

- Errors occurring when the machine is used as a LAN-Fax will not be displayed on the computer. Check for errors by using Web Image Monitor. See Web Image Monitor help.

- It is recommended that you use Web Image Monitor running under the same network environment as this machine. Otherwise, the Web browser may not open and an error may occur.

- This function supports both IPv4 and IPv6 addresses.

Related topics

Before Use
Using the Software
Installing Individual Applications
Setting LAN-Fax Driver Properties
Basic Transmission
Specifying Options
Checking Transmission Using LAN-Fax Driver
Confirming Transmission Results by E-mail
LAN-Fax Result Report
Printing and Saving
Editing Address Book
Editing Fax Cover Sheets
Managing Facsimile Functions Using SmartDeviceMonitor for Admin
Using the Machine's Address Book as the LAN-Fax Destination List
LAN-Fax Operation Messages