ManualsContentsPreviousNext
Settings

# Confirming by Report

Print reports for confirmation.

Memory Transmission

You can confirm the result with a Communication Result Report.

This report is printed each time a Memory Transmission is completed if turned on with User Parameter (switch 03, bit 0) in the Facsimile Features menu.

You can also print the report by programming the TX Status Report to a Quick Operation Key and pressing this when specifying a destination.

If you turn the Communication Result Report on, the Communication Failure Report is not printed.

For details about the contents printed in the reports, see “Communication Result Report (Memory Transmission)” or “Communication Failure Report”.

Immediate Transmission

You can confirm the result with an Immediate TX Result Report.

Select to print this report in User Parameter (switch 03, bit 5) in the Facsimile Features menu. A report is printed after every Immediate Transmission is completed.

You can also print the report by programming the TX Status Report to a Quick Operation Key and pressing this when specifying a destination.

For details about the contents printed in the report, see “Immediate TX Result Report (Immediate Transmission)”.

- For details about Parameter Setting, see “Parameter Settings”.

- For details about Quick Operation Key, see “General Settings”.

- Communication Result Report (Memory Transmission)

- Immediate TX Result Report (Immediate Transmission)

- Communication Failure Report

- General Settings

- Parameter Settings