ManualsContentsPreviousNext
Settings

# Confirming Transmission Results by E-mail

Use this function to confirm the transmission results by sending an e-mail notification to the specified destination.

- Register the e-mail address of the destination for e-mail notification in the destination list in advance.

Place the original, and then select the scan settings you require.

Specify the sender.

For details, see “Sender Settings”.

Press [TX Mode].

Press [E-mail TX Results].

Select the destination of notification, and then press [OK].

If you make a mistake, before pressing [OK], press [Clear] or press the selected Destination key again to turn the highlight off.

[E-mail TX Results] gets highlighted and the destination of notification selected appears.

Press [OK].

The standby display appears.

To check the settings, press [TX Mode].

Specify a destination, and then press the [Start] key.

- You can program one of the Quick Operation keys with operations for this function. Using the Quick Operation Key allows you to omit steps 3 and 6. For details about Quick Operation Key, see “General Settings”.

- Sender Settings

- General Settings