| ManualsContentsPreviousNext |

# Interface Settings

This section describes how to make Interface settings using utilities.

Change settings by using Web Image Monitor and telnet.

[Network] [Machine IPv4 Address] [Auto-Obtain (DHCP)]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Machine IPv4 Address] [Specify] "Machine IPv4 Address"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Machine IPv4 Address] [Specify] "Subnet Mask"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [IPv4 Gateway Address]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Machine IPv6 Address] "Manual Configuration Address"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [IPv6 Gateway Address]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [IPv6 Stateless Address Autoconfiguration]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [DNS Configuration] [Auto-Obtain (DHCP)]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [DNS Configuration] [Specify] "DNS Server 1-3"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [DDNS Configuration]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [IPsec]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Domain Name] [Auto-Obtain (DHCP)]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Domain Name] [Specify] "Domain Name"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [WINS Configuration] [On] "Primary WINS Server"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [WINS Configuration] [On] "Secondary WINS Server"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [WINS Configuration] [On] "Scope ID"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [WINS Configuration] [Off]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Effective Protocol] "IPv4"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Effective Protocol] "IPv6"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Effective Protocol] "NetWare"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Effective Protocol] "SMB"

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NCP Delivery Protocol] [IPX Priority]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NCP Delivery Protocol] [TCP / IP Priority]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NCP Delivery Protocol] [IPX Only]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NCP Delivery Protocol] [TCP / IP Only]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NW Frame Type] [Auto Select]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NW Frame Type] [Ethernet II]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NW Frame Type] [Ethernet 802.2]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NW Frame Type] [Ethernet 802.3]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [NW Frame Type] [Ethernet SNAP]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [SMB Computer Name]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [SMB Work Group]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Ethernet Speed]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Cannot be used for specifying the setting.

[Network] [IEEE 802.1X Authentication for Ethernet]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [LAN Type] [Ethernet]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [LAN Type] [Wireless LAN]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Ping Command]

- Web Image Monitor: Cannot be used for specifying the setting.

- telnet: Cannot be used for specifying the setting.

[Network] [Permit SNMPv3 Communication] [Encryption Only]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Permit SNMPv3 Communication] [Encryption / Cleartext]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Permit SSL / TLS Communication] [Ciphertext Only]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Cannot be used for specifying the setting.

[Network] [Permit SSL / TLS Communication] [Ciphertext Priority]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Cannot be used for specifying the setting.

[Network] [Permit SSL / TLS Communication] [Ciphertext / Cleartext]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Cannot be used for specifying the setting.

[Network] [Host Name]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Machine Name]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Network] [Restore IEEE 802.1X Authentication to Defaults]

- Web Image Monitor: Cannot be used for specifying the setting.

- telnet: Cannot be used for specifying the setting.

[Wireless LAN] [Communication Mode] [802.11 Ad-hoc Mode]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Wireless LAN] [Communication Mode] [Infrastructure Mode]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Wireless LAN] [SSID Setting]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Wireless LAN] [Ad-hoc Channel]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.

[Wireless LAN] [Security Method]

- Web Image Monitor: Can be used for specifying the setting.

- telnet: Can be used for specifying the setting.