| ManualsContentsPreviousNext |

# When P is displayed

This section describes how to remove misfeeds from location “P”.

1. Open the upper cover of the ADF.

2. Remove the misfed paper.

3. Open the right cover of the ADF.

4. Remove the misfed paper.

5. Close the right and upper cover of the ADF.

6. Lift the ADF.

7. Turn the knob P, and then remove the misfed paper.

   1. Knob P

8. Lower the ADF.