ManualsContentsPreviousNext
Settings

# diprint

The direct printing port enables direct printing from a network-connected computer.

Use the "diprint" command to change direct printing port settings.

View settings

The following command displays the current direct printing port settings:

`msh> diprint`

Example output:

`port 9100`

`timeout=300(sec)`

`bidirect on`

`conn multi`

`apl async`

- The "port" specifies the port number of the direct printing port.

- The "bidirect" setting indicates whether the direct printing port is bidirectional or not.

Bidirectional communication settings

`msh> diprint bidirect {on|off}`

- The default is "on".

Setting timeout

`msh> diprint timeout [30-65535]`

- You can specify the timeout interval to use when the printer is expecting data from the network.

- The default is 300 seconds.

- This command functions in conjunction with the "lpr" command.

Specifying the number of concurrent connections

`msh> diprint conn {multi|single}`

- The above command specifies the number of concurrent diprint connections. Specify "multi" for multiple connections or "single" for a single connection.

- The default is "multi".