ManualsContentsPreviousNext
Settings

# Unusable Paper

This section describes paper unusable on this machine.

| Do not attempt to print on stapled sheets, aluminum foil, carbon paper, or any kind of conductive paper. Doing so risks fire.

- To prevent faults, do not use any of the following kinds of treated paper:

  - Paper for inkjet printers

  - Thermal fax paper

  - Art paper

  - Aluminum foil

  - Carbon paper

  - Conductive paper

  - Paper with perforated lines

  - Hemmed-edge paper

  - OHP transparencies for color copying

  - Window envelopes

- Faults can occur if you copy or print onto sides that are already printed. Take care to copy or print onto unprinted sides only.

- To prevent misfeeds, do not use the following kinds of paper:

  - Bent, folded, or creased paper

  - Perforated paper

  - Slippery paper

  - Torn paper

  - Rough paper

  - Thin paper with little stiffness

  - Paper with a dusty surface

- Even supported types of paper may cause paper jams or malfunctions if the paper is not in good condition.

- If you copy or print onto rough grain paper, the output image might be blurred.

- Do not load sheets that have already been printed onto by another machine. (Sheets can become jammed if they have been improperly stored.)