ManualsContentsPreviousNext
Settings

# Wireless LAN

This section lists the settings required for using the printer or LAN-Fax function with a wireless LAN connection.

For details about how to specify the settings, see "Interface Settings".

Menu | User Tool | Setting Requirements
--- | --- | ---
Interface Settings/Network | Machine IPv4 Address | Necessary
Interface Settings/Network | IPv4 Gateway Address | As required
Interface Settings/Network | Machine IPv6 Address | As required
Interface Settings/Network | IPv6 Gateway Address | As required
Interface Settings/Network | IPv6 Stateless Address Autoconfiguration | As required
Interface Settings/Network | DNS Configuration | As required
Interface Settings/Network | DDNS Configuration | As required
Interface Settings/Network | IPsec | As required
Interface Settings/Network | Domain Name | As required
Interface Settings/Network | WINS Configuration | As required
Interface Settings/Network | Effective Protocol | Necessary
Interface Settings/Network | NCP Delivery Protocol | As required
Interface Settings/Network | NW Frame Type | As required
Interface Settings/Network | SMB Computer Name | As required
Interface Settings/Network | SMB Work Group | As required
Interface Settings/Network | LAN Type | Necessary
Interface Settings/Network | Permit SNMPv3 Communication | As required
Interface Settings/Network | Permit SSL / TLS Communication | As required
Interface Settings/Network | Host Name | As required
Interface Settings/Network | Machine Name | As required
Interface Settings/Wireless LAN | Communication Mode | Necessary
Interface Settings/Wireless LAN | SSID Setting | As required
Interface Settings/Wireless LAN | Ad-hoc Channel | As required
Interface Settings/Wireless LAN | Security Method | As required

- For the Effective Protocol setting, check that the protocol you want to use is set to [Active].

- [Wireless LAN] and [LAN Type] are displayed when the wireless LAN board is installed. If both Ethernet and wireless LAN are connected, the selected interface takes precedence.

- Interface Settings