| ManualsContentsPreviousNext |

# Cleaning the Registration Roller

This section describes how to clean the registration roller.

If the registration roller is dirty, a misfeed might occur or dots (caused by specks of paper stuck to the roller) appear on printed OHP transparencies. In this case, clean the roller as follows:

| Be sure to turn off the power switch and wait for about 15 minutes before cleaning the registration roller. Not waiting for the machine to cool down can result in a burn.

1. Turn off the main power switch, and then unplug the power plug.

2. Push the button on the right side of the machine to open the front cover.

3. Hold the print cartridge's front handle to lift and pull it out.

4. Wipe around the metallic registration roller by turning with a soft damp cloth. After that, wipe it with a dry cloth to remove the moisture.

5. Hold the grips of the cartridge, and then insert it into the machine until it stops.

6. Close the front cover.