ManualsContentsPreviousNext
Settings

# Programming Initial Set Up of a Special Sender

This section describes how to program Initial Set Up of a Special Sender.

Program the “Initial Set Up” of a Special Sender. You can also specify the Bypass Tray Paper Size.

Press [Facsimile Features].

Press [Reception Settings].

Press [Program Special Sender].

Press [Initial Set Up].

Select the function you want to program.

To program Authorized Reception and Special Reception Function, press [Authorized Reception] or [Special Reception Function].

Press [On] or [Off], and then press [OK].

The illustration shows the “Authorized Reception” display as an example.

To program Bypass Tray Paper Size, press [Bypass Tray Paper Size].

Select the size you want to program.

You can select a size from [Regular Size], or [Custom Size].

If you select [Regular Size], proceed to step 10.

If you select [Custom Size], proceed to step 11.

Select the size you want to program from the sizes shown.

After selecting the size, proceed to step 14.

Make sure that [Vertical] is selected.

Enter the vertical size of the paper using the number keys, and then press [].

Specify a vertical size from 140 mm (5.6 inches) to 900 mm (35.4 inches).

Each time you press [mm] or [inch], the units switch between “mm” and “inch”.

If you enter a length and change the units by pressing [mm] or [inch], it is converted automatically (fractions are rounded off).

Enter the horizontal size of the paper using the number keys, and then press [].

Specify a horizontal size from 64 mm (2.6 inches) to 216 mm (8.5 inches).

Each time you press [mm] or [inch], the units switch between “mm” and “inch”.

If you enter a length and change the units by pressing [mm] or [inch], it is converted automatically (fractions are rounded off).

Press [OK].

Press [Exit].

Press the [User Tools/Counter] key.