ManualsContentsPreviousNext
Settings

# Locating Jammed Paper

A misfeed has occurred in the place corresponding to the letter displayed on the control panel.

Press the key of the section from where you want to remove the jammed paper.

After each step is complete, press [Next]. To go back to the previous step, press [Previous].

When all jammed paper is removed, restore the machine to the original state.

- More than one misfeed may be indicated. When this happens, check all the areas indicated.

- If there is no misfed paper in the first area you check, see the other areas that are indicated.