ManualsContentsPreviousNext
Settings

# Simultaneous transmission

The following table tells you the maximum values of settings for using the E-mail and Scan to Folder functions simultaneously.

Values of Set Items for Simultaneous transmission

Item | Maximum value | Comments
--- | --- | ---
Number of destinations you can select for E-mail and Scan to Folder | 550 addresses |
Number of destinations you can select for sending by e-mail | 500 addresses | You can specify a maximum of 100 directly entered destinations, including LDAP search-retrieved destinations.
Number of destinations you can set for sending by Scan to Folder | 50 addresses |