ManualsContentsPreviousNext
Settings

# Order of Option Installation

When installing multiple options, the following order is recommended:

Attach the paper feed unit.

Attach the paper feed unit to the bottom of the machine.

You can attach up to three paper feed units. Up to 2300 sheets of paper can be loaded in total.

For details, see “Installing the Paper Feed Unit (Optional)”.

Install the optional board.

Install the Gigabit Ethernet board, Wireless LAN interface unit, or File Format Converter in the slot.

For details, see “Installing the Board (Optional)”.

Insert SD card options.

Insert the browser unit into the SD card slot.

If you want to use two or more SD cards that can be inserted in the same slot, contact your sales and service representative.

For details, see “Installing the SD Card (Optional)”.

- Installing the Paper Feed Unit (Optional)

- Installing the Board (Optional)

- Installing the SD Card (Optional)