| ManualsContentsPreviousNext |

# Unpacking

To protect it from shock and vibration during transit, this machine comes packaged in cushioning foam and secured with tape. Remove these protective materials after bringing the machine to where it will be installed.

| Keep the polythene materials (bags, gloves, etc.) supplied with this machine away from babies and small children at all times. Suffocation can result if polythene materials are brought into contact with the mouth or nose.

| Do not remove any covers or screws other than those explicitly mentioned in this manual. Inside this machine are high voltage components that are an electric shock hazard and laser components that could cause blindness. Contact your sales or service representative if any of the machine's internal components require maintenance, adjustment, or repair. Do not attempt to disassemble or modify this machine. Doing so risks burns and electric shock. Note again that exposure to the laser components inside this machine risks blindness.

| Do not incinerate toner (new or used) or toner containers. Doing so risks burns. Toner will ignite on contact with naked flame.

| Do not place the machine on an unstable or tilted surface. If it topples over, an injury might occur.

| Type 1 weighs approximately 45 kg (99.2 lb.), type 2 weighs approximately 47 kg (103.7 lb.), and type 3 weighs approximately 52 kg (114.7 lb.). When moving the machine, use the inset grips on both sides, and lift slowly. The machine will break or cause injury if dropped.

| Do not crush or squeeze toner containers. Doing so can cause toner spillage, possibly resulting in dirtying of skin, clothing, and floor, and accidental ingestion.

| Store toner (new or used), toner containers, and components that have been in contact with toner out of reach of children.

| If toner or used toner is inhaled, gargle with plenty of water and move into a fresh air environment. Consult a doctor if necessary.

| If toner or used toner gets into your eyes, flush immediately with large amounts of water. Consult a doctor if necessary.

| If toner or used toner is swallowed, dilute by drinking a large amount of water. Consult a doctor if necessary.

- Removed tape is dirty. Be careful not to let it touch your hands or clothes.

- Leave the tape holding the paper tray and cover in place while moving the machine.

- Do not grip on the tray area when lifting the machine.

- Do not allow small objects such as paper clips to fall into or become stuck inside the machine.

- Keep the uncovered print cartridge away from direct sunlight.

- When you use this machine for the first time, use the print cartridge packaged with the machine.

1. Remove the plastic bag.

2. Lift the machine by the inset grips on its sides.

   At least four people are needed to lift the machine.

3. Lower the machine slowly and carefully to prevent trapping your hands.

4. Remove the adhesive tape attached on the machine's exterior.

5. Carefully pull out tray 1 (type 3 only).

6. Remove the extender from tray 1 (type 3 only).

7. Carefully push tray 1 fully in (type 3 only).

8. Attach the extender to the finisher tray (type 3 only).

9. Lift the ADF.

10. Remove the protective material attached on the exposure glass.

11. Lower the ADF.

12. Push the button on the right side of the machine to open the front cover.

13. Hold the print cartridge's front handle to lift and pull it out.

    Place the print cartridge on a stable, flat surface.

14. Remove the protective material attached on the machine's interior.

15. Hold the grips of the cartridge, and then insert it into the machine until it stops.

16. Close the front cover.

- Print cartridges (consumables) are not covered by warranty. However, if there is problem, contact the store where they were purchased.

- The actual machine may come with protective materials attached in different positions. Make sure to check the machine for all protective materials, and remove them completely.