| ManualsContentsPreviousNext |

# Combined Copying

This section describes how to make combined copies.

- When placing originals on the exposure glass, start with the first page to be copied. When placing originals in the ADF, set the first page on top.

- When placing originals on the exposure glass or in the ADF using the Batch function, press the [] key after all the originals have been scanned.

- If you selected [2 Sided] for Original or [Combine 2 Sides] for Copy, you can change the orientation. See “Originals and Copy Orientation”.

- You can change the initial settings for 1-Sided Combine or 2-Sided Combine under Edit in User Tools. For details, see “Edit”.

- In this mode, the machine selects the reproduction ratio automatically. This reproduction ratio depends on copy paper sizes and the number of originals.

- The machine selects reproduction ratios of between 25 and 400%. However, if the originals are placed in the ADF, the maximum reproduction ratio is 200%. To copy originals at reproduction ratio above 200%, you must place them on the exposure glass.

- If the calculated ratio is under the minimum ratio, it is automatically adjusted to within available range. However, with some ratios, parts of the image might not be copied.

- Depending on the orientation of the original and copy paper, the machine will automatically rotate the image by 90 degrees to make copies properly.

- If the number of originals placed is less than the number specified for combining, the last page segment is left blank as shown.

- Originals and Copy Orientation

- Edit

Related topics

One-Sided Combine
Two-Sided Combine