| ManualsContentsPreviousNext |

# Detecting Blank Sheet

Upon completion of the first page scanning, an alarm sounds if the page is nearly blank.

- The blank sheet-detecting function works only when an original is scanned using the ADF.

- The blank sheet-detecting function is ineffective for second and subsequent pages.

- The machine cannot detect blank sheets if the user has put it into Preview mode using [Preview].

This function notifies you if an original is placed wrong side down on the scanner. When this happens, a message appears for a few seconds. The message differs depending on number of pages to be scanned and transmission mode.

- When sending a document using Immediate Transmission or when all pages have been scanned in Memory Transmission:

- When some pages are left unscanned in Parallel Memory Transmission or Memory Transmission:

- Even if a near blank sheet is detected, it is transmitted as normal.

- You can turn this function on or off with the User Parameter (switch 11, bit 2). See “Parameter Settings”.

- To cancel scanning if a blank sheet is detected, press the [Clear/Stop] key.

- Parameter Settings