ManualsContentsPreviousNext
Settings

# If There Is No Paper of the Correct Size

If there is no paper in the machine that matches the size of a received document, the machine will choose a paper size based on the paper available.

This function is available only if the following settings are made:

- Reduction in Sub-scan Direction: Enabled

- Page Separation Threshold: 20 mm (0.79 inches)

- Width or Length Priority: Width

If you have not set the same size paper in the paper tray, incoming fax documents are printed on the nearest size available.

(mainly Europe and Asia)

For example, if your machine does not have A5 loaded and you receive an A5 size document, the document is printed on A4. If your machine does not have A4 loaded and you receive an A4 size document, the document is printed on two sheets of A5.

(mainly North America)

For example, if your machine does not have 81/2 × 11 loaded and you receive an 81/2 × 11 size document, the document is printed on 81/2 × 14. If your machine does not have 81/2 × 14 loaded and you receive an 81/2 × 14 size document, the document is printed on two sheets of 81/2 × 11.

- The document is split over two sheets of paper depending on the paper size. See “Page Separation and Length Reduction”.

- Paper placed in the bypass tray is not usually selected for printing a received document. However, you can use this tray if you select the bypass tray as the main paper tray using Reception with Specified Senders.

- Widths that this machine can receive are A4 and 81/2 × 11. Any documents narrower than A4 or 81/2 × 11 are received at A4 or 81/2 × 11 width. The length of documents depends on the document.

- The paper size used to print a received document may be different from the size of the sent original.

- Page Separation and Length Reduction

Related topics

Setting priority trays
Just size printing
Having incoming documents printed on paper from the bypass tray