ManualsContentsPreviousNext
Settings

# autonet

Use the "autonet" command to configure AutoNet parameters.

View settings

The following command displays the current AutoNet settings:

`msh> autonet`

Configuration

You can configure AutoNet settings.

`msh> autonet {on|off}`

- {on} means "active" and {off} means "inactive".

Current interface priority configuration display

`msh> autonet priority`

Interface priority configuration

`msh> autonet priority "interface_name"`

- You can give interface's AutoNet parameter priority.

- Priority settings are available when multiple interfaces are installed.

- wlan can be specified only when the IEEE 802.11 interface is installed.

Interface | Interface configured
--- | ---
ether | Ethernet interface
wlan | IEEE 802.11 interface

- If an interface is not selected, the current interface connection settings remain in effect.