ManualsContentsPreviousNext
Settings

# snmp

Use the "snmp" command to display and edit the SNMP configuration settings such as the community name.

View settings

"IPX" is shown only when the NetWare is installed.

`msh> snmp`

- Default access settings 1 is as follows:

  Community name:public

  IPv4 address:0.0.0.0

  IPv6 address:::

  IPX address:00000000:000000000000

  Access type:read-only

  Effective Protocol:IPv4/IPv6/IPX

- Default access settings 2 is as follows:

  Community name:admin

  IPv4 address:0.0.0.0

  IPv6 address:::

  IPX address:00000000:000000000000

  Access type:read-write

  Effective Protocol:IPv4/IPv6/IPX

- If "-p" is added, you can view settings one by one.

- To display the current community, specify its registration number.

Display

`msh> snmp ?`

Community name configuration

`msh> snmp "number" name "community_name"`

- You can configure ten SNMP access settings numbered 1-10.

- The printer cannot be accessed from SmartDeviceMonitor for Admin or SmartDeviceMonitor for Client if “public” is not registered in numbers 1-10. When changing the community name, use SmartDeviceMonitor for Admin and SNMP Setup Tool to correspond with printer settings.

- The community name can be entered using up to 15 characters.

Deleting community name

`msh> snmp "number" clear name`

Access type configuration

`msh> snmp "number" type "access_type"`

Access type | Type of access permission
--- | ---
no | not accessible
read | read only
write | read and write
trap | user is notified of trapmessages

Protocol configuration

Use the following command to set protocols "active" or "inactive". If you set a protocol "inactive", all access settings for that protocol are disabled.

"IPX" is shown only when the NetWare is installed.

`msh> snmp {ipv4|ipv6|ipx} {on|off}`

- Specify "ipv4" for IPv4, "ipv6" for IPv6, or "ipx" for IPX/SPX.

- {on} means "active" and {off} means "inactive".

- All protocols cannot be turned off concurrently.

Configuration of protocol for each registration number

"IPX" is shown only when the NetWare is installed.

`msh> snmp "number" active {ipv4|ipv6|ipx} {on|off}`

- To change the protocol of access settings, use the following command. However, if you have disabled a protocol with the above command, activating it here has no effect.

Access configuration

"IPX" is shown only when the NetWare is installed.

`msh> snmp "number" {ipv4|ipv6|ipx} "address"`

- You can configure a host address according to the protocol used.

- The network interface board accepts requests only from hosts that have IPv4, IPv6, and IPX addresses with access types of "read-only" or "read-write". Enter "0" to have the network interface board accept requests from any host without requiring a specific type of access.

- Enter a host address to deliver "trap" access type information to.

- To specify IPv4 or IPv6, enter "ipv4" or "ipv6" followed by a space, and then the IPv4 or IPv6 address.

- To specify IPX/SPX, enter "ipx" followed by a space, the IPX address followed by a decimal, and then the MAC address of the network interface board.

sysLocation configuration

`msh> snmp location "character string"`

Deleting sysLocation

`msh> snmp clear location`

sysContact setting

`msh> snmp contact "character string"`

Deleting sysContact

`msh> snmp clear contact`

SNMP v1v2 function configuration

`msh> snmp v1v2 {on|off}`

- Specify "on" to enable, and "off" to disable.

SNMP v3 function configuration

`msh> snmp v3 {on|off}`

- Specify "on" to enable, and "off" to disable.

SNMP TRAP configuration

`msh> snmp trap {v1|v2|v3} {on|off}`

- Specify "on" to enable, and "off" to disable.

Remote configuration authorization configuration

`msh> snmp remote {on|off}`

- Specify "on" to enable, and "off" to disable the SNMP v1v2 setting.

SNMP v3 TRAP configuration display

`msh> snmp v3trap`

`msh> snmp v3trap [1-5]`

- If a number from 1 to 5 is entered, settings are displayed for that number only.

Configuring a sending address for SNMP v3 TRAP

"IPX" is shown only when the NetWare is installed.

`msh> snmp v3trap [1-5] {ipv4|ipv6|ipx} "address"`

Configuring a sending protocol for SNMP v3 TRAP

"IPX" is shown only when the NetWare is installed.

`msh> snmp v3trap [1-5] active {ipv4|ipv6|ipx} {on|off}`

Configuring a user account for SNMP v3 TRAP

`msh> snmp v3trap [1-5] account "account_name"`

- Enter an account name using up to 32 alphanumeric characters.

Deleting an SNMP v3 TRAP user account

`msh> snmp v3trap [1-5] clear account`

Configuring an SNMP v3 encryption algorithm

`msh> snmp v3auth {md5|sha1}`

Configuring SNMP v3 encryption

`msh> snmp v3priv {auto|on}`

- Set "auto" for automatic encryption configuration.

- If you select "on", plain-text communication becomes impossible - only encrypted communication is possible.

- "Encrypted communication" means an encrypted password is set on the machine.

- To use SNMP Setup Tool, you must first download SmartDeviceMonitor for Admin from the manufacturer's Web site and install it on your computer. Contact your local dealer for information on downloading SmartDeviceMonitor for Admin.