ManualsContentsPreviousNext
Settings

# Configuring the WINS Server

This section explains configuring the WINS server.

The printer can be configured to register its NetBIOS name with a WINS server when the power is turned on. This enables the NetBIOS name of the printer to be specified from SmartDeviceMonitor for Admin even in a DHCP environment.

- WINS servers are supported by Windows Server 2003 or later.

- For details about the WINS server settings, see Windows Help.

- If there is no reply from the WINS server, the NetBIOS name is registered by broadcast.

- The NetBIOS name can be entered using up to 15 alphanumeric characters.

Related topics

Using Web Image Monitor
Using telnet