| ManualsContentsPreviousNext |

# To add new receiver

Use Web Image Monitor to add a new destination to the Address Book.

1. Start a Web browser.

2. Enter “http://(IPv4 address, IPv6 address or host name of this machine)/” in the address bar.

   The top page of Web Image Monitor is displayed.

3. Click [Login], and then enter the Administrator's name and password.

4. Click [Address Book] in the left pane.

   The Address Book is displayed.

5. Click [Add User].

   The [Add User] page appears.

6. Enter the registration number, name, and e-mail address, then set the necessary properties.

   You can set the Internet Fax data format after entering the e-mail address.

7. Click [Full Mode] under [Internet Fax Data Format], and set the properties according to the receiver's properties.

   If you change the mode to “Simple Mode”, you cannot set machine properties.

8. Click [OK] at the upper or lower left of the screen.

   To cancel the setting, click [Cancel] at the upper or lower left of the screen.

   The Address Book is displayed.

9. Close the Web browser.