| ManualsContentsPreviousNext |

# Connecting to the Ethernet Interface (mainly Europe and Asia)

This section describes how to connect an Ethernet cable to the Ethernet interface.

Caution:

A network interface cable with a ferrite core must be used for RF interference suppression.

- If the main power switch is on, turn it off.

- Use the following Ethernet cables:

  - Unshielded Twisted Pair Cable (UTP) or Shielded Twisted Pair Cable (STP) and Category type 5 or more

1. A ferrite core for the Ethernet interface cable is supplied with this machine. Attach the ferrite core at the machine end of the Ethernet cable.

2. Make sure the main power is switched off.

3. Connect the Ethernet interface cable to the 10BASE-T/100BASE-TX port.

4. Connect the other end of the Ethernet interface cable to a network connection device such as a hub.

5. Turn on the main power switch of the machine.

   1. Indicators

      When 100BASE-TX or 10BASE-T is operating, the green LED is lit and the orange LED flashes. If the machine is not connected to the network, both LEDs are turned off.

- For details about how to turn on the main power switch, see "Turning On/Off the Power", About This Machine.

- For details about installing the printer driver, see "Preparing the Machine", Printer Reference.