ManualsContentsPreviousNext
Settings

# Setting Items of IEEE 802.1X for Ethernet

Log in to Web Image Monitor in the administrator mode.

In the menu area, click [Configuration].

Under "Security", click [IEEE 802.1X].

In "User Name", enter the user name set in the RADIUS server.

Enter the domain name in "Domain Name".

Select "EAP Type". Configurations differ according to the EAP Type.

EAP-TLS

- Make the following settings according to the operating system you are using:

  - Select [On] or [Off] in "Authenticate Server Certificate".

  - Select [On] or [Off] in "Trust Intermediate Certificate Authority".

  - Enter the host name of the RADIUS server on "Server ID".

  - Select [On] or [Off] in "Permit Sub-domain".

LEAP

- Click [Change] in "Password", and then enter the password set in the RADIUS server.

EAP-TTLS

- Click [Change] in "Password", and then enter the password set in the RADIUS server.

- Click [Change] in "Phase 2 User Name", and then enter the user name set in the RADIUS server.

- Select [CHAP], [MSCHAP], [MSCHAPv2], [PAP], or [MD5] in "Phase 2 Method".

  Certain methods might not be available, depending on the RADIUS server you want to use.

- Make the following settings according to the operating system you are using:

  - Select [On] or [Off] in "Authenticate Server Certificate".

  - Select [On] or [Off] in "Trust Intermediate Certificate Authority".

  - Enter the host name of the RADIUS server in "Server ID".

  - Select [On] or [Off] in "Permit Sub-domain".

PEAP

- Click [Change] in "Password", and then enter the password set in the RADIUS server.

  If [TLS] is selected for "Phase 2 Method", you do not need to specify a password.

- Click [Change] on "Phase 2 User Name", and then enter the user name set in the RADIUS server.

- Select [MSCHAPv2] or [TLS] in "Phase 2 Method".

  When you select [TLS], you must install "IEEE 802.1X Client Certificate".

- Make the following settings according to the operating system you are using:

  - Select [On] or [Off] in "Authenticate Server Certificate".

  - Select [On] or [Off] in "Trust Intermediate Certificate Authority".

  - Enter the host name of the RADIUS server on "Server ID".

  - Select [On] or [Off] in "Permit Sub-domain".

Click [OK].

`“Updating...”` appears. Wait for about one or two minutes, and then click [OK].

In the menu area, click [Configuration].

Under "Interface", click [Interface Settings].

Select [Active] in "Ethernet Security".

Click [OK].

`“Updating...”` appears. Wait for about one or two minutes, and then click [OK].

Click [Logout].

Quit the Web Image Monitor.

- If there is a problem with settings, you might not be able to communicate with the printer. To identify the problem, print a network summary.

- If you cannot identify the problem, reset the printer interface to normal, and then repeat the procedure from the beginning.