ManualsContentsPreviousNext
Settings

# Displaying the destination prior to transmission

To prevent documents being sent to the wrong destination, you can configure the machine to display the destination again after it has been entered and before the file is sent.

If you want to enable this function, contact your service representative.

Note that the entered destination will not be displayed again if you are sending the fax by any of the following means:

- Scanning without entering a destination (storing documents, storing documents in Information Boxes)

- On Hook Dial

- Manual Dial

- the simplified display

Specify the destination.

If you make a mistake, press the [Clear/Stop] key, and then enter the number again.

Press the [Start] key.

Displays the destination and the transmission settings.

To change the destination, press [Exit], and then specify the destination again.

Press the [Start] key again.

Transmission starts.

After transmission, the standby display appears.