| ManualsContentsPreviousNext |

# Parallel Memory Transmission

This function dials while the original is being scanned.

Standard Memory Transmission stores the original in memory, and then dials the destination. However, Parallel Memory Transmission allows you to confirm the connection status quickly. In addition, this function scans the original faster than Immediate Transmission. This is useful when you are in a hurry and need to use the original for another purpose.

- Standard Memory Transmission is used instead of Parallel Memory Transmission in the following cases:

  - When the line is busy and could not be connected to

  - With Send Later

  - When you store an original for Memory Transmission while another communication is in progress

  - When two or more destinations are specified

  - When an original is placed on the exposure glass, and then sent

  - When you send documents stored in the Document Server

  - When the machine has been switched to the Preview mode with [Preview].

- You can turn this function on or off with the User Parameter (switch 07, bit 2) in the Facsimile Features menu. See “Parameter Settings”.

- Standard Memory Transmission may be used instead of Parallel Memory Transmission depending on the optional equipment installed if there is not enough free memory left.

- If you use this function, the Memory Storage Report will not be printed.

- If the [Clear/Stop] key is pressed, the original jams or memory runs out, Parallel Memory Transmission will stop. The Communication Result Report is printed and files are deleted.

- When using Parallel Memory Transmission, only the page number is printed on the header of the fax, the total number of originals is not automatically printed.

- Parameter Settings