ManualsContentsPreviousNext
Settings

# Specifications

Fax Transmission and Reception

Component | Specifications
--- | ---
Standard | G3
Resolution | G3: 8 × 3.85 lines/mm, 200 × 100 dpi (Standard character), 8 × 7.7 lines/mm, 200 × 200 dpi (Detail character), 8 × 15.4 lines/mm (Fine character: optional), 16 × 15.4 lines/mm, 400 × 400 dpi (Super Fine character: optional)
Transmission time | G3: 3 seconds at 28,800 bps, Standard resolution (JBIG transmission: 2 seconds)
Data compression method | MH, MR, MMR, JBIG
Maximum original size | Standard: A4, 81/2 × 14 Custom: 210 × 1,200 mm, 81/2 × 47 inches
Maximum scanning size | 210 × 1,200 mm, 81/2 × 47 inches
Print process | Printing on standard paper using a laser
Transmission speed | G3: 33,600 / 31,200 / 28,800 / 26,400 / 24,000 / 21,600 / 19,200 / 16,800 / 14,400 / 12,000 / 9,600 / 7,200 / 4,800 / 2,400 bps (auto shift down system)

Power Consumption

Component | Specifications
--- | ---
Immediate Transmission | Approx. 230 W
Memory Transmission | Approx. 220 W
Memory Reception | Approx. 220 W
Reception | Approx. 600 W

IP-Fax Transmission and Reception

Component | Specifications
--- | ---
Network | Standard: Ethernet interface (100BASE-TX/10BASE-T) Optional: Gigabit Ethernet interface (1000BASE-T/100BASE-TX/10BASE-T) IEEE 802.11a/b/g wireless LAN interface
Scan line density | 8 × 3.85 lines/mm, 200 × 100 dpi (Standard character), 8 × 7.7 lines/mm, 200 × 200 dpi (Detail character), 8 × 15.4 lines/mm (Fine character: optional), 16 × 15.4 lines/mm, 400 × 400 dpi (Super Fine character: optional)
Maximum original size | Standard: A4, 81/2 × 14 Custom: 210 × 1,200 mm, 81/2 × 47 inches
Maximum scanning size | 210 × 1,200 mm, 81/2 × 47 inches
Transmission protocol | Recommendation: T.38, TCP, UDP/IP communication, SIP (RFC 3261 compliant), H.323 v2
Compatible machines | IP-Fax compatible machines
IP-Fax transmission function | Specify an IP address and send faxes to an IP-Fax compatible fax through a network. Also capable of sending faxes to a G3 fax connected to a telephone line via a VoIP gateway.
IP-Fax reception function | Receive faxes sent from an IP-Fax compatible fax through a network. Also capable of receiving faxes from a G3 fax connected to a telephone line via a VoIP gateway.

Internet Fax Transmission and Reception

Component | Specifications
--- | ---
Network | Standard: Ethernet interface (100BASE-TX/10BASE-T) Optional: Gigabit Ethernet interface (1000BASE-T/100BASE-TX/10BASE-T) IEEE 802.11a/b/g wireless LAN interface
Transmit function | E-mail
Scan line density | 200 × 100 dpi (Standard character), 200 × 200 dpi (Detail character), 200 × 400 dpi (Fine character: optional)*1, 400 × 400 dpi (Super Fine character: optional)*1
Original size : Scanning width | A4
Communication Protocols | Transmission SMTP, TCP/IP Reception POP3, SMTP, IMAP4, TCP/IP
E-mail format | Single/Multi-part, MIME Conversion Attached file forms: TIFF-F (MH, MR*1, MMR*1 compression)
Authentication method | SMTP-AUTH, POP before SMTP, A-POP
Internet communication | Send and receive e-mail with a computer that has an e-mail address.
Encryption method (for forwarding) | S/MIME
Internet Fax send functions | Automatic conversion of sent documents to e-mail format and e-mail transmission. Memory transmission only.
Internet Fax receive functions | Automatic detection and printing of appended TIFF-F (MH) files and ASCII text. Memory reception only.

*1 Full mode

E-mail Transmission and Reception, and Folder Transmission

Component | Specifications
--- | ---
Network | Standard: Ethernet interface (100BASE-TX/10BASE-T) Optional: Gigabit Ethernet interface (1000BASE-T/100BASE-TX/10BASE-T) IEEE 802.11a/b/g wireless LAN interface
Scan line density | 200 × 100 dpi (Standard character)*1, 200 × 200 dpi (Detail character), 400 × 400 dpi (Super Fine character: optional)
Maximum original size | Standard: A4, 81/2 × 14 Custom: 210 × 1,200 mm, 81/2 × 47 inches
Maximum scanning size | 210 × 1,200 mm, 81/2 × 47 inches
E-mail reception/transmission protocols | Transmission SMTP, TCP/IP Reception (Mail to Print) POP3, SMTP, IMAP4, TCP/IP
Protocols for sending files to folders | SMB, FTP, NCP, TCP/IP
E-mail formats | Single/Multi-part, MIME Conversion
File formats | Transmission TIFF (MH, MR, MMR compression), PDF Reception (Mail to Print) JPEG (JFIF), PDF
Authentication methods | SMTP-AUTH, POP before SMTP, A-POP
Encryption method (for forwarding) | S/MIME
E-mail sending functions | Automatically converts documents to e-mail format and sends them as e-mail.
E-mail receiving functions | Automatically detects and prints JPEG and PDF documents attached to received e-mail.
Sending to folder functions | Sends scanned files over the network to shared folders, FTP server folders, or NetWare folders.

*1 When you send document in TIFF format.

Related topics

Specifications Required for the Internet Fax Destination Machines