ManualsContentsPreviousNext
Settings

# Specifications

Specifications
Component | Specifications
--- | ---
Type | Full-color scanner
Scan method | Flatbed scanning
Image sensor type | CCD Image Sensor
Scan type | Sheet, book, three-dimensional object
Original sizes that can be scanned | Length 140 355 mm (51/2 14 inches) Width 128 216 mm (5 81/2 inches)
Scan speed | When using the E-mail/Scan to Folder/WSD(Push Type)/Scan to Removable device/network delivery scanner function (Original size: A4, Resolution: 200 dpi, 1-side scanning): Black and white: 30 pages/min (Original Type: B & W: Text / Line Art, Compression (Black & White): MH, ITU-T No1 Chart) Full Color: 30 pages/min (Original Type: Full Colour: Text / Photo, Compression (Grey Scale / Full Colour): Default, Original Chart) Scanning speed differs depending on the following; operating environment of the machine and computer, scan settings, and the content of originals (denser images require more time).
Tone | Black and white: 2 tones Full color / Gray scale: 256 tones
Basic scanning resolution | 600 dpi
Image compression type for black and white (two-value) | TIFF (MH, MR, MMR)
Image compression type for gray scale/full color | JPEG
Interface | Standard: Ethernet interface (100BASE-TX/10BASE-T) Option: Gigabit Ethernet interface (1000BASE-T/100BASE-TX/10BASE-T) IEEE 802.11a/b/g wireless LAN interface
Network protocol | TCP/IP
Selectable scanning resolutions when using the E-mail function (main scanning × sub scanning) | 100 dpi, 200 dpi, 300 dpi, 400 dpi, 600 dpi
Protocol for sending e-mail | SMTP, SMTPS, POP3
Sendable file formats when using the E-mail function | TIFF, JPEG, PDF, High Compression PDF
Selectable scanning resolutions when using the Scan to Folder function (main scanning × sub scanning) | 100 dpi, 200 dpi, 300 dpi, 400 dpi, 600 dpi
Protocol for Scan to Folder | SMB, FTP, NCP
Sendable file formats when using the Scan to Folder function | TIFF, JPEG, PDF, High Compression PDF
Protocol for sending using WSD | Web Services on Devices for scanning
Selectable scanning resolution when using TWAIN scanner (main scanning × sub scanning) | When using the exposure glass: 100 to 1200 dpi When using the ADF: 100 to 600 dpi
Protocol for TWAIN scanner | TCP/IP
Operating system for TWAIN scanner | Windows XP/Vista/7, Windows Server 2003/2003 R2/2008/2008 R2 (Operates in 32-bit compatibility mode on 64-bit operating systems)
Selectable scanning resolutions when using the network delivery scanner function (main scanning × sub scanning) | 100 dpi, 200 dpi, 300 dpi, 400 dpi, 600 dpi
Selectable scanning resolutions when using WIA scanner (main scanning × sub scanning) | When using the exposure glass: 100 to 1200 dpi When using the ADF: 100 to 600 dpi
Protocol for WIA scanner | TCP/IP
Operating system for WIA scanner | Windows Vista (SP1 or later)/7, Windows Server 2008/2008 R2 (WIA scanner can function under both 32- and 64-bit operating systems.)

- Specifications are subject to change without notice.