| ManualsContentsPreviousNext |

# To set label insertion

This section describes how to set label insertion.

When Label Insertion is set to On, the receiver's name and standard messages are printed on the fax message when it is received at the other end.

1. Press [Change] under "Label Insertion".

2. Press [On].

3. Press [Change] under "Line 2".

4. Select the new standard message or press [Manual Entry] to enter the new message.

5. If you selected “Manual Entry” in step 4, enter the new message, and then press [OK].

6. Press [OK].

7. Press [Change] under "Line 3".

8. Select the new standard message, and then press [OK].

9. Press [OK].

- To change the name, key display and title, see "Registering Names".

- Registering Names