| ManualsContentsPreviousNext |

# Installing the TWAIN Driver from the Supplied CD-ROM

This section explains how to install the TWAIN driver on a client computer from the supplied CD-ROM.

To use the network TWAIN scanner, you must install the TWAIN driver on a client computer.

1. Start Windows, and then insert the CD-ROM into the CD-ROM drive of the client computer.

   The installer starts.

2. Select an interface language, and then click [OK].

3. Click [TWAIN Driver].

4. The installer of the TWAIN driver starts. Follow the instructions.

- Before you start the installation, check the system requirements for the TWAIN driver. For details about the system requirements, see "Software Supplied on CD-ROM".

- You can install the software using the auto-run program. For details about the auto-run program, see "Auto-Run Program".

- If the installer does not start automatically, see "Auto-Run Program".

- When the installation is complete, a message about restarting the client computer may appear. In this case, restart the client computer.

- After the installation is complete, a folder with the name of the machine in use is added in [Programs] or [All Programs] on the [Start] menu. Help can be displayed from here.

- Notes on using the network TWAIN scanner are provided in "Readme.txt". Be sure to read them before use.

- Software Supplied on CD-ROM

- Auto-Run Program