| ManualsContentsPreviousNext |

# Specifications Required for the Internet Fax Destination Machines

This section explains the specifications required for the Internet Fax destination machine.

When communicating with full mode-compatible machines, you can take advantage of higher specifications for coding, original size, and resolution. For details about the specifications available in full mode, see “Internet Fax Transmission and Reception” in “Specifications”.

Component | Specifications
--- | ---
Communication protocols | Transmission SMTP Reception POP3, SMTP, IMAP4
E-mail format | Format MIME, Base64 Content-Type Image/tiff Multipart/mixed (text/plain, Image/tiff (attached file forms))
Data format | Profile TIFF Profile S Coding MH Original size A4 Resolution (dpi) 200 × 100/200 × 200, 204 × 98/204 × 196

- Specifications