ManualsContentsPreviousNext
Settings

# Setting Custom Size Paper Using the Control Panel

Follow the procedure below to set the machine using the control panel when loading custom size paper onto the bypass tray.

- If you select [Machine Setting(s)] in [Bypass Tray] under [Tray Setting Priority] in [System] of [Printer Features], the settings made using the control panel have priority over the printer driver settings. For details about [System] settings, see "System".

Press the [User Tools/Counter] key on the control panel.

Press [System Settings].

Press the [Tray Paper Settings] tab.

Press [Printer Bypass Paper Size].

Press [Custom Size].

If a custom size is already set, press [Change Size].

Press [Vertical], enter the vertical size of the paper using the number keys, and then press [].

Press [Horizontal], enter the horizontal size of the paper using the number keys, and then press [].

Press [OK].

The paper sizes entered are displayed.

Press [OK].

Press the [User Tools/Counter] key.

The initial screen appears.

- When loading thick paper, thin paper or OHP transparencies, set paper size and paper type.

- The default paper size for the bypass tray is as follows:

  - (mainly Europe and Asia)

    A4

  - (mainly North America)

    81/2 × 11

- For details about setting printer drivers, see the printer driver Help.

- System