| ManualsContentsPreviousNext |

# Entering a destination directly

This section explains how to enter a destination manually.

1. Click the [Specify Destination] tab.

   The [Specify Destination] tab appears.

2. Select the type of fax from the [Type:] dropdown menu.

   To send by standard fax or IP-Fax, select [Fax]. To send by Internet Fax, select [E-mail].

   After you select the fax type, the items corresponding to the selected type appear.

3. Specify the destination.

   Specify the destination depending on the selected fax type as follows:

   - If you selected [Fax]: enter the fax number. To send by IP-Fax, enter the IP-Fax destination.

   - If you selected [E-mail]: enter the e-mail address.

   To enter a pause in the fax number, click [Pause]. If you selected [E-mail] in step 2, [Pause] is not available.

4. Specify settings according to the type of fax transmission.

   Specify settings according to the type of fax transmission selected in step 2, as follows:

   - If you selected [Fax], select a line or a protocol in the [Line:] list.

   - If you selected [E-mail], select the [Do not use SMTP server] check box if you want to bypass the SMTP server.

5. Click [Set as Destination].

   The entered destination is added and appears in the [List of Destination:] box.

   If you add a destination by mistake, click the wrong destination, and then click [Delete from List].

6. To specify more destinations, repeat steps 2 through 5.

- For details about specifying destinations, see the LAN-Fax Driver's Help.

- For the maximum number of digits that can be included in a destination, see “Maximum Values”.

- Maximum Values