| ManualsContentsPreviousNext |

# Connecting to the Wireless LAN Interface

This section describes how to connect to the wireless LAN interface.

- Check the machine's IPv4 address and subnet mask, or the IPv6 address settings.

- For details about how to set the IPv4 address and subnet mask from the control panel of the machine, see "Interface Settings".

- Before using this machine with a wireless LAN interface, you must select [Wireless LAN] in [LAN Type].

- Interface Settings

Related topics

Setup Procedure
Checking the signal