ManualsContentsPreviousNext
Settings

# Communication Failure Report

This report is printed when a document could not be successfully transmitted with Memory Transmission.

If the machine is set up to print a Communication Result Report, this report is not printed. Use it to keep a record of failed transmissions so you can send them again.

- You can select whether the Communication Failure Report is automatically printed using the User Parameter (switch 04, bit 1) in the Facsimile Features menu.

- This report is only printed if the Communication Result Report is turned off and a document could not be successfully transmitted with Memory Transmission.

- You can select whether to include part of the original image on the report with the User Parameter (switch 04, bit 7) in the Facsimile Features menu.

- If user authentication is set, you can select whether to display a destination with the User Parameter (switch 04, bit 4) in the Facsimile Features menu.

- If user authentication is set, you can select whether to display a sender name with the User Parameter (switch 04, bit 5) in the Facsimile Features menu.

- For details about Parameter Setting, see “Parameter Settings”.

- The Pg(s) column gives the total number of pages. The Page Not Sent column gives the number of pages that could not be sent successfully.

- “Unprogrammed” indicates that the document could not be sent because the forwarding destination is not programmed.

- “--” indicates that the e-mail or Internet Fax document was sent to the mail server programmed in this machine. (However, this does not mean the e-mail was delivered.)

- Parameter Settings