ManualsContentsPreviousNext
Settings

# Edit

This section describes the user tools in the Edit menu under Copier / Document Server Features.

Enter the width of the binding margin with the number keys as follows:

- (mainly Europe and Asia)

  0 30 mm (in increments of 1 mm)

- (mainly North America)

  0.0 1.2 inches (in increments of 0.1 inches)

Enter the width of the erased margin with the number keys as follows:

- (mainly Europe and Asia)

  2 99 mm (in increments of 1 mm)

- (mainly North America)

  0.1 3.9 inches (in increments of 0.1 inches)

An image of approximately 1.5 mm (0.06 inches) will not be displayed as the width of the separation line, when specifying solid or broken lines.

Front Margin: Left / Right

Specify left and right margins on the front side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[Left: 5 mm]

(mainly North America)

[Left: 0.2 inch]

Back Margin: Left / Right

Specify left and right margins on the back side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[Right: 5 mm]

(mainly North America)

[Right: 0.2 inch]

Front Margin: Top / Bottom

Specify top and bottom margins on the front side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[T / B: 0 mm]

(mainly North America)

[T / B: 0.0 inch]

Back Margin: Top / Bottom

Specify top and bottom margins on the back side of copies in Margin Adjustment mode.

Default:

(mainly Europe and Asia)

[T / B: 0 mm]

(mainly North America)

[T / B: 0.0 inch]

1 Sided 2 Sided Auto Margin: TtoT

In 1 sided 2 sided Duplex mode, you can specify the margins on the back side.

The margin is set to the same value of “Back Margin: Left/Right”.

Default:

(mainly Europe and Asia)

[Right: 5 mm]

(mainly North America)

[Right: 0.2 inch]

1 Sided 2 Sided Auto Margin: TtoB

In 1 sided 2 sided Duplex mode, you can specify the margins on the back side.

The value set for “Back Margin: Top/Bottom” is used.

Default:

(mainly Europe and Asia)

[T / B: 0 mm]

(mainly North America)

[T / B: 0.0 inch]

Erase Border Width

Specify the width for erasing border.

Default:

(mainly Europe and Asia)

[1 0 mm]

(mainly North America)

[0.4 inch]

Erase Original Shadow in Combine

In Combine mode, you can specify whether to erase a 3 mm, 0.1 inches boundary margin around all four edges of each original.

Default: [On]

Erase Centre Width

Specify the width of the erased center margins with this function.

Default:

(mainly Europe and Asia)

[1 0 mm]

(mainly North America)

[0.4 inch]

Front Cover Copy in Combine

You can make a combined copy on the front cover sheet when you select Front Cover mode.

Default: [Combine]

Copy Order in Combine

You can set the copy order in Combine mode to From Left to Right or From Top to Bottom.

Default: [From Left to Right]

Orientation: Booklet, Magazine

Select the opening orientation of copies made using Booklet or Magazine mode.

Default: [Open to Left]

Copy on Designating Page in Combine

Specify whether to make a combined copy on the inserted slip sheets in Designate/Chapter mode.

Default: [Combine]

Image Repeat Separation Line

You can select a separation line using the Image Repeat function from: None, Solid, Broken A, Broken B, or Crop Marks.

1. None

2. Solid

3. Broken A

4. Broken B

5. Crop Marks

Default: [None]

Selecting solid or broken lines might produce a blank area of approximately 1.5 mm (0.06 inches) in width along the separation line.

Separation Line in Combine

You can select a separation line using the Combine function from: None, Solid, Broken A, Broken B, or Crop Marks.

1. None

2. Solid

3. Broken A

4. Broken B

5. Crop Marks

Default: [None]

Selecting solid or broken lines might produce a blank area of approximately 1.5 mm (0.06 inches) in width along the separation line.