ManualsContentsPreviousNext
Settings

# Basic Procedure for Sending Scan Files Using WSD (Pull Type)

This section explains the basic procedure for sending scan files using WSD (Pull Type).

On the client computer, click the [Start] menu, point to [All Programs], and then click [Windows Fax and Scan].

Place an original on this machine.

In the [Windows Fax and Scan] window, click the [File] menu, point to [New], and then click [Scan...].

If a dialog box for selecting the device you want to use appears, select the name of the device in the list, and then click [OK].

The [New Scan] dialog box appears.

Make settings for the type of original, type of scanning, and orientation of the original, etc.

For details, see "Scan Profile Items and Settings".

In the [New Scan] dialog box, click [Scan].

The original is scanned.

Send the scan data by e-mail as an attachment or save it as a file.

- If scanning takes too long, the computer might time out and display the error message "Automatic Scanning could not be completed" on the computer screen. If this happens, change the scan settings or scan the originals one side at a time.

- In the profile settings, if you select [Feeder (Scan one side)] for [Source], only one side will be scanned per operation. If you select [Feeder (Scan both sides)] for [Source], two sides will be scanned per operation.

- When scanning from the ADF, you must click [Scan] in the [New Scan] dialog box each time you scan an original.

- You cannot scan originals while other originals are being scanned.

- Two-sided originals are scanned for sideways opening (top-to-top orientation).

- Transmission results of WSD scanning (Pull Type) jobs do not appear in File Status.

- The Blank Page Detect function is not available when you are using the WSD scanner (Pull Type).

- If scanning is not at the specified size, delete the scan profile, and then scan again. For details about deleting a scan profile, see "Changing a Scan Profile".

- To scan an original correctly, place it as shown in the following table:

  Placing an original
  Scanning method (Exposure glass/ADF) | Original orientation
  --- | ---
  Exposure glass | top corner touching top left corner of exposure glass
  Auto Document Feeder (ADF) | top edge leading

- Scan Profile Items and Settings

- Changing a Scan Profile

- Enabling WSD using Web Image Monitor